EDL Instruction Interface - valid Reason Codes

­

DD MMM 2023

**Contents**

[1. Introduction 3](#_Toc88743063)

[2. Valid Reason Code combinations 4](#_Toc88743064)

[Appendix A – Document Information 7](#_Toc88743065)

1. Introduction

## Overview

This document has been produced as a guide for external organisations developing

EDL NETA Software. It details the valid reason codes that may be sent from NGESO to

control points via EDL. The operational interpretation of any payment associated with

these codes can be found in the relevant Ancillary Services Contract. For a complete

set of technical EDL specifications refer to NETA Project EDL Message Interface

Specification CT/24.13.0013.

1. Valid Reason Code combinations

## Conventional rotating plant (Inc Hydro)

DNS – Cease Contracted Response Service(s) Note this does not remove the grid code obligation to provide Limited Frequency Sensitive Response.

DC – Dynamic Containment Response

DCL – Dynamic Containment Low Response

DCH – Dynamic Containment High Response

DM - Dynamic Moderation Response

DML – Dynamic Moderation Low Response

DMH – Dynamic Moderation High Response

DR – Dynamic Regulation Response

DRL – Dynamic Regulation Low Response

DRH – Dynamic Regulation High Response

ITA – Intertrip Service Armed

ITD – Intertrip Service Disarmed

MN – Limited Frequency Sensitive Response

MF – Primary, Secondary and High Frequency Response

MP – Primary and High Frequency

MFA – Primary, Secondary and High Frequency Response Subject to ASB contract A

MFB – Primary, Secondary and High Frequency Response Subject to ASB contract B

MFC – Primary, Secondary and High Frequency Response Subject to ASB contract C

MFD – Primary, Secondary and High Frequency Response Subject to ASB contract D

MFE – Primary, Secondary and High Frequency Response Subject to ASB contract E

MPA – Primary and High Frequency Response Subject to ASB contract A

MPB – Primary and High Frequency Response Subject to ASB contract B

MPC – Primary and High Frequency Response Subject to ASB contract C

MPD – Primary and High Frequency Response Subject to ASB contract D

MPE – Primary and High Frequency Response Subject to ASB contract E

EN – Emergency Instruction

BN – Instruction Logged due to Participants Behest

MR – Commence Fast Reserve Service

MO – Cease Fast Reserve Service

MNS – Limited Frequency Sensitive (Normal Slow Start or Normal Off)

MNV – Synch comp reason code

VQV – Start static reactive power service

VQO – Cease static reactive power service

Please visit [https://www.nationalgrideso.com/balancing-services/lio-eic-codes](https://www.nationalgrideso.com/balancing-services/lio-eic-codes%20) for information on EIC codes and application forms to apply for EIC codes.

The EIC codes you will require will be W and/or X.

Please contact [Box.lio@nationalgrideso.com](file:///C:\Users\angela.j.wilks\AppData\Local\Microsoft\Windows\INetCache\Content.Outlook\WEZDW1MJ\Box.lio@nationalgrideso.com) for all EIC related enquiries.

Appendix A – Document Information

### Document Author

**Author: Stuart Brace, System Change Manager, NGESO**

### Document Amendment History:

|  |  |  |  |
| --- | --- | --- | --- |
| **Version** | **Date** | **Amended By** | **Remarks** |
| 2.0 | 23 Jul 2001 | Neil Ashley | Issued for NETA go-live |
| 3.0 | 1 Jan 2021 | John Walsh | Updated to reflect EDL for Stability Pathfinder instructions |
| 4.0 | 22Oct 2021 | Angela Wilks | Updated to add new reason code for static reactive power service for Long Term Mersey Voltage Pathfinder |
| 5.0 | 20 Jan 2022 | Stuart Brace | Updated to add EDL disarming/re-arming instructions for Dynamic Moderation, Dynamic Regulation and Dynamic Containment |
| 6.0 | 24 Oct 2022 | Haarith Dhorat | Updated to add new reason codes for intertrip service |

Faraday House, Warwick Technology Park, Gallows Hill, Warwick, CV346DA

nationalgrideso.com