Starting point was “1955 - legal review - CMP315 original Charging v1.37 6 October 2022 anonymised.docx” including the on the fly changes last workgroup 5th December

Aspects to note :

In the FIRST year for each variant, do we smooth in the new value over last year’s CMP353 (RPI on 2020/21) value using alpha = 0.13, or do we jump direct to the new value and only apply alpha in subsequent years ? I have assumed in the text that the proposers all want that, to avoid a step change in year 1. This is 14.15.71 in the texts for 315 and 375, and 14.15.77 in the text for the WACM. Easy to remove if any proposer doesn’t want that.

Note from 14.15.59, in all texts, that “*Reinforcements to existing circuits that add neither life nor capacity, will be ignored*”. As otherwise the £/MW/km will come out as infinity.

Also here it is set out that for reinforcements, account is taken of the remaining asset life prior to the investment, and of the new remaining asset life after the investment *(needed for the “shapes” legal text, which Paul Jones provided after the last meeting; in the legal text for CMP315/75, this is found at 14.15.65, or at 14.15.72 for the WACM).* A defaulting rule is set out, also in 14.15.59 : “*For any investment for which the Transmission Owner is unable to give The Company the remaining life before the investment, a default assumption of 0 years of remaining life will be applied. For any investment for which the Transmission Owner is unable to give The Company the remaining life after the investment was made, a default assumption of 45 years of remaining life will be applied*”.

The old 14.15.79A “Onshore Expansion Factors in RIIO-T2” text was describing CMP353, and had to go. I overlooked that in the 5th December text.

**14th April edition – note of new changes :**

Replied to legal query in comment box re : 14.14.5 (iv) – made no change to text

14.15.4 changed instance of MWkm to £/MW/km as per prompt from legal; removed “(Reinforcements to existing circuits that add neither life nor capacity, will be ignored).”, as, as legal point out, this is also said in 14.15.59, and 14.15.4 is meant to be a high level initial introductory description of charging prior to more details

Each instance of “per MW per km” replaced with “£/MW/km” for consistency

14.15.59 “Transmission Owner” is not actually a defined term in section 11 (it only has offshore Transmission Owner, and Onshore Transmission Licensee), so Transmission Owner cannot be in bold and I’ve instead now said **Onshore Transmission Licensee**

14.15.62 erroneously still said “, normalised against the 400KV overhead line (OHL) figure”, I removed that.

All references in 14.15.65 to “Investment Cost” changed to “investment cost”.

All references to NGET capitalised, as it’s a defined term in Section 11

“Offshore Transmission Owner” un-capitalised in 14.15.87

Nick Silitto added 3 terms to 14.15.5

Nick Sillito supplied new formula for 14.15.65 (c) for annuity factor, the result of mine was mathematically OK but having WACC as a denominator to the denominator was dumb and pointless, flip it and make it the numerator ….

At the end of 14.15.69, added after a meeting with Nick Sillito “The circuit length of the non-circuit elements will be based on the average for that voltage level of the data submitted by the Transmission Owners|”

Deleted all of old 14.15.68 as that (about what WACC is) was already in 14.15.65 part C. Renumbered subsequent sections.

"charging website” in 14.15.67 about overhead factor, changed to “the charging details to be found on **The Company Website”**

Checked paragraph numbers as last step :

In para 14.15.62, the reference to paras 14.15.74-83 was corrected to 14.15.73-87

1. 14.15.63 now refers to which data is used to (changed bit shows in bold) “**perform the calculation in 14.15.65 and thereby populate inputECnewk in 14.15.66”**

14.15.65 – paragraph reference here corrected to 14.15.63

14.15.66 – removed reference to WACC here, as the WACC/annuity factor step was done as part of the steps within 14.15.65.

Updated 14.15.66’s reference to overhead factor (which is as at 14.15.67), updated text in 14.15.67 .

14.15.67 now refers to 14.15.68

**26th May edition – note of new changes :**

As requested at 2nd May workgroup meeting, removed all comment boxes

Deleted all of 14.15.61 “The transmission infrastructure capital costs used in the calculation of the expansion constant are provided via an externally audited process. They also include information provided from all onshore Transmission Owners (TOs). They are based on historic costs and tender valuations adjusted by a number of indices (e.g. global price of steel, labour, inflation, etc.). The objective of these adjustments is to make the costs reflect current prices, making the tariffs as forward looking as possible. This cost data represents The Company’s best view; however it is considered as commercially sensitive and is therefore treated as confidential. The calculation of the expansion constant also relies on a significant amount of transmission asset information, much of which is provided in the Seven Year Statement.”

Reference corrections:

Reference in 14.15.62 to 14.15.65,66 corrected to 14.15.64,65

Reference in 14.15.63 to 14.15.65,66 corrected to 14.15.64,65

Reference in 14.15.64 to 14.15.63,64 corrected to 14.15.62,63

Reference in 14.15.65 to 14.15.67 corrected to 14.15.66

27th June – jumped to version 26 to match latest version number of CMP375, skipping a couple of version numbers.

– as discussed at the WG meeting 22nd June, paras 14.15.62 and 63 have been changed, the change showing in yellow (yellowing of changes prior to 22nd June has been removed), to make sure that inflation is applied to the last 10 years data when the calculation is first performed and to the last year’s data in subsequent years. This indexation had been omitted. These suggested changes by ESO to the legal text of this CMP315 are subject to the proposer’s consent as he missed the WG.

I mentioned at the last CMP375 WG meeting on 22nd June, I felt in the light of the new project by project approach to gathering TO data under CMP315/375/WACM2, compared to aggregated TO data by asset class under baseline, there needed to be changes to the paragraphs that in this text are numbered 14.15.72 and 14.15.73, deleting the former paragraph 14.15.72 that shows here as deleted 14.15.69. These changes show in yellow, including the deleted former paragraph 14.15.72. Comments explain the changes. These suggested changes by ESO to the legal text of this CMP315 are subject to the proposer’s consent (flagged to him Monday). Also deleted here the meaningless para that said “the 400 kV onshore circuit expansion constant is applied on a GB basis and reflects the full costs for 400 kV cable and overhead lines”

# Part 2 - The Statement of the Use of System Charging Methodology

# Section 1 – The Statement of the Transmission Use of System Charging Methodology

# 14.14 Principles

1. Transmission Network Use of System charges reflect the cost of installing, operating and maintaining the transmission system for the Transmission Owner (TO) Activity function of the Transmission Businesses of each Relevant Transmission Licensee. These activities are undertaken to the standards prescribed by the Transmission Licences, to provide the capability to allow the flow of bulk transfers of power between connection sites and to provide transmission system security.
2. A Maximum Allowed Revenue (MAR) defined for these activities and those associated with pre-vesting connections is set by the Authority at the time of the Transmission Owners’ price control review for the succeeding price control period. Transmission Network Use of System Charges are set to recover the Maximum Allowed Revenue as set by the Price Control (where necessary, allowing for any Kt adjustment for under or over recovery in a previous year net of the income recovered through pre-vesting connection charges).
3. The basis of charging to recover the allowed revenue is the Investment Cost Related Pricing (ICRP) methodology, which was initially introduced by The Company in 1993/94 for England and Wales. The principles and methods underlying the ICRP methodology were set out in the The Company document "**Transmission Use of System Charges Review: Proposed Investment Cost Related Pricing for Use of System (30 June 1992)"**.
4. In December 2003, The Company published the Initial Thoughts consultation for a GB methodology using the England and Wales methodology as the basis for consultation. The Initial Methodologies consultation published by The Company in May 2004 proposed two options for a GB charging methodology with a Final Methodologies consultation published in August 2004 detailing The Company’s response to the Industry with a recommendation for the GB charging methodology. In December 2004, The Company published a Revised Proposals consultation in response to the Authority’s invitation for further review on certain areas in The Company’s recommended GB charging methodology.
5. In April 2004 The Company introduced a DC Loadflow (DCLF) ICRP based transport model for the England and Wales charging methodology. The DCLF model has been extended to incorporate Scottish network data with existing England and Wales network data to form the GB network in the model. In April 2005, the GB charging methodology implemented the following proposals:
6. The application of multi-voltage circuit expansion factors with a forward-looking Expansion Constant that did not include substation costs in its derivation.
7. The application of locational security costs, by applying a multiplier to the Expansion Constant reflecting the difference in cost incurred on a secure network as opposed to an unsecured network.
8. The application of a de-minimis level demand charge of £0/kW for Half Hourly and £0/kWh for Non Half Hourly metered demand to avoid the introduction of negative demand tariffs.
9. The application of 132kV expansion factor on a Transmission Owner basis reflecting the regional variations in network upgrade plans.
10. The Company will set tariffs in a manner so that the locational varying element, as established by the DCLF ICRP model and, where appropriate, local substation and local circuit charges, are levied on all Generator and Demand Users. Any remaining Transmission Owner revenues will be recovered from demand only in a non-locational manner through a residual charge.
11. For the purpose of compliance with the Limiting Regulation in the context of setting limits on the annual charges paid by generation The Company will exclude Charges for Physical Assets Required for Connection when calculating the total amount to be recovered from Generators (GCharge (Forecast)).
12. If having applied the exclusion of Charges for Physical Assets Required for Connection The Company identifies that an adjustment to TNUoS Charges is required to remain compliant with the Limiting Regulation then an Adjustment Tariff will be applied to all Generators in the following circumstances.

i.) The Adjustment Tariff will be applied if The Company identifies that either:

a. Annual average TNUoS charges payable by Generator Users will fall below €0/MWh

OR

b. Annual average TNUoS charges payable by Generator Users will exceed €2.50/MWh adjusted by a risk margin to allow for error in tariff setting.

ii.) Where annual average TNUoS charges to Generators are positive under the GCharge (Forecast) the Adjustment Tariff will be applied if the Adjustment Revenue is less than £0. The Adjustment Revenue is expressed as:

𝐴𝑑𝑗𝑅𝑒𝑣𝑒𝑛𝑢𝑒 = (𝐺𝑂 ∗ ((𝐶𝑎𝑝𝐸𝐶 ∗ (1 − 𝑦)) ∗ 𝐸𝑅)) –

𝐺𝐶ℎ𝑎𝑟𝑔𝑒(𝐹𝑜𝑟𝑒𝑐𝑎𝑠𝑡)

1. Where annual average TNUoS charges to Generators are negative under the GCharge (Forecast) the Adjustment Revenue will be the difference between £0 and the total recovered from Generators. The Adjustment Revenue will be expressed as:

𝐴𝑑𝑗𝑅𝑒𝑣𝑒𝑛𝑢𝑒 = 0 − 𝐺𝐶ℎ𝑎𝑟𝑔𝑒(𝐹𝑜𝑟𝑒𝑐𝑎𝑠𝑡)

1. The total adjusted revenue expected to be recovered from Generators (AdjGenRev) through TNUoS tariffs can therefore be expressed as:

𝐴𝑑𝑗𝐺𝑒𝑛𝑅𝑒𝑣 = 𝐺𝐶ℎ𝑎𝑟𝑔𝑒(𝐹𝑜𝑟𝑒𝑐𝑎𝑠𝑡) + 𝐴𝑑𝑗𝑅𝑒𝑣𝑒𝑛𝑢𝑒

1. The error margin used in calculating TNUoS tariffs for the **Financial Year** is expressed as:

y = (1+ ErrorGenRev) / (1 - ErrorGO) -1

1. Where:

**y** = error margin expressed in %.

**ErrorGenRev** = the highest absolute percentage error in generation revenue collection, adjusted by systemic error, from the past 5 full years (year t-6 to t-2 inclusive). Systemic error is the average of %error in generation revenue collection for the past 5 full years. Systemic error can be positive or negative.

**ErrorGO** = the highest absolute percentage error in generation TWh outputs, from the past 5 full years (year t-6 to t-2 inclusive).

1. The Company will use the latest OBR Forecast of £/€ exchange rate published prior to the 31st October in the year preceding the relevant **Financial Year** to convert average annual TNUoS charges payable by Generators in the GCharge (Forecast) to a comparable value for the purposes of assessing compliance with the Limiting Regulation.
2. The Adjustment Tariff used in the calculation will be either:

1. a negative £/kW tariff that reduces annual average TNUoS charges to Generators to below the risk adjusted upper limit of the Limiting Regulation in accordance with 14.14.5 (vi).

OR

2. a positive £/kW tariff that increases annual average TNUoS charges to Generators to above the lower limit of the Limiting Regulation in accordance with 14.14.5 (vi).

Expressed in either case as:

𝐴𝑑𝑗𝑇𝑎𝑟𝑖𝑓𝑓 = 𝐴𝑑𝑗𝑅𝑒𝑣𝑒𝑛𝑢𝑒

𝐶ℎ𝑎𝑟𝑔𝑒𝑎𝑏𝑙𝑒𝐶𝑎𝑝𝑎𝑐𝑖𝑡y

Where;

CapEC = Upper limit of the range specified in the Limiting Regulation

y = Error margin built in to adjust CapEC

GO = Forecast GB Generation Output for generation liable for Transmission charges (i.e. energy injected into the transmission network in MWh) for the **Financial Year**

ER = The latest OBR Forecast €/£ Exchange Rate published prior to the 31st October in the year preceding the relevant **Financial Year**

GCharge (Forecast) =The total forecast TNUoS revenue to be recovered from Generators in the **Financial Year** minus Charges for Physical Assets Required for Connection.

AdjRevenue = Adjustment Revenue

Chargeable Capacity = as per paragraph 14.18.6

AdjTariff = Any Adjustment Tariff required to remain compliant with the Limiting Regulation.

1. The currently applicable number of generation zones, determined in accordance with 14.15.37 and using the criteria outlined in paragraph 14.15.42, is detailed in **The Company’s Statement of Use of System Charges** which is available from the **Charging website** and has been determined as 27.
2. The number of demand zones has been determined as 14, corresponding to the 14 GSP groups.
3. The underlying rationale behind Transmission Network Use of System charges is that efficient economic signals are provided to Users when services are priced to reflect the incremental costs of supplying them. Therefore, charges should reflect the impact that Users of the transmission system at different locations would have on the Transmission Owner's costs, if they were to increase or decrease their use of the respective systems. These costs are primarily defined as the investment costs in the transmission system, maintenance of the transmission system and maintaining a system capable of providing a secure bulk supply of energy.

The Transmission Licence requires The Company to operate the National Electricity Transmission System to specified standards. In addition The Company with other transmission licensees are required to plan and develop the National Electricity Transmission System to meet these standards. These requirements mean that the system must conform to a particular Security Standard and capital investment requirements are largely driven by the need to conform to both the deterministic and supporting cost benefit analysis aspects of this standard. It is this obligation, which provides the underlying rationale for the ICRP approach, i.e. for any changes in generation and demand on the system, The Company must ensure that it satisfies the requirements of the Security Standard.

1. The Security Standard identifies requirements on the capacity of component sections of the system given the expected generation and demand at each node, such that demand can be met and generators’ output over the course of a year (capped at their Transmission Entry Capacity, TEC) can be accommodated in the most economic and efficient manner. The derivation of the incremental investment costs at different points on the system is therefore determined against the requirements of the system both at the time of peak demand and across the remainder of the year. The Security Standard uses a Demand Security Criterion and an Economy Criterion to assess capacity requirements. The charging methodology therefore recognises both these elements in its rationale.
2. The Demand Security Criterion requires sufficient transmission system capacity such that peak demand can be met through generation sources as defined in the Security Standard, whilst the Economy Criterion requires sufficient transmission system capacity to accommodate all types of generation in order to meet varying levels of demand efficiently. The latter is achieved through a set of deterministic parameters that have been derived from a generic Cost Benefit Analysis (CBA) seeking to identify an appropriate balance between constraint costs and the costs of transmission reinforcements.
3. The TNUoS charging methodology seeks to reflect these arrangements through the use of dual backgrounds in the Transport Model, namely a Peak Security background representative of the Demand Security Criterion and a Year Round background representative of the Economy Criterion.
4. To recognise that various types of generation will have a different impact on incremental investment costs the charging methodology uses a generator’s TEC, Peak Security flag, and Annual Load Factor (ALF) when determining Transmission Network Use of System charges relating to the Peak Security and Year Round backgrounds respectively. For the Year Round background the diversity of the plant mix (i.e the proportion of low carbon and carbon generation) in each charging zone is also taken into account.
5. In setting and reviewing these charges The Company has a number of further objectives. These are to:

* offer clarity of principles and transparency of the methodology;
* inform existing Users and potential new entrants with accurate and stable cost messages;
* charge on the basis of services provided and on the basis of incremental rather than average costs, and so promote the optimal use of and investment in the transmission system; and
* be implementable within practical cost parameters and time-scales.

1. Condition C13 of the Transmission Licence governs the adjustment to Use of System charges for small generators. Under the condition, The Company is required to reduce TNUoS charges paid by eligible small generators by a designated sum, which will be determined by the Authority. The licence condition describes an adjustment to generator charges for eligible plant, and a consequential change to demand charges to recover any shortfall in revenue. The mechanism for recovery will ensure revenue neutrality over the lifetime of its operation although it does allow for effective under or over recovery within any year. For the avoidance of doubt, Condition C13 does not form part of the Use of System Charging Methodology.
2. The Company will typically calculate TNUoS tariffs annually, publishing final tariffs in respect of a **Financial Year** by the end of the preceding January. However The Company may update the tariffs part way through a **Financial Year**.

# 14.15 Derivation of the Transmission Network Use of System Tariff

1. The Transmission Network Use of System (TNUoS) Tariff comprises two separate elements. Firstly, a locationally varying element derived from the DCLF ICRP transport model to reflect the costs of capital investment in, and the maintenance and operation of, a transmission system to provide bulk transport of power to and from different locations. Secondly, a non-locationally varying element related to the provision of residual revenue recovery from demand only. The combination of both these elements forms the TNUoS tariff.
2. For generation TNUoS tariffs the locational element itself is comprised of five separate components. Three wider components –

* Wider Peak Security Component
* Wider Year Round Not-shared component
* Wider Year Round component

These components reflect the costs of the wider network under the different generation backgrounds set out in the Demand Security Criterion (for Peak Security component) and Economy Criterion (for both Year Round components) of the Security Standard. The two Year Round components reflect the unshared and shared costs of the wider network based on the diversity of generation plant types.

Two local components –

* Local substation, and
* Local circuit

These components reflect the costs of the local network.

Accordingly, the wider tariff represents the combined effect of the three wider locational tariff components and the local tariff represents the combination of the two local locational tariff components.

Finally, an Adjustment Tariff component may also be charged to Generators as per paragraph 14.14.5.

1. The process for calculating the TNUoS tariff is described below.

## The Transport Model

### **Model Inputs**

1. The DCLF ICRP transport model calculates the marginal costs of investment in the transmission system which would be required as a consequence of an increase in demand or generation at each connection point or node on the transmission system, based on a study of peak demand conditions using both Peak Security and Year Round generation backgrounds on the transmission system. One measure of the investment costs is in terms of £/MW/km. This is the concept that ICRP uses to calculate marginal costs of investment. The investment may take the form of entire new circuits, or may take the form of reinforcements of existing circuits to add additional capacity, or add asset life.Hence, marginal costs are estimated initially in terms of increases or decreases in units of kilometres (km) of the transmission system for a 1 MW injection to the system.
2. The transport model requires a set of inputs representative of the Demand Security and Economy Criterion set out in the Security Standards. These conditions on the transmission system are represented in the Peak Security and Year Round background respectively as follows:

* Nodal generation information per node (TEC, plant type and SQSS scaling factors)
* Nodal net demand information
* Transmission circuits between these nodes
* The associated lengths of these routes, the proportion of which is overhead line or cable and the respective voltage level

The £/MW/km expansion costs in for each of 132kV overhead line, 132kV underground cable, 275kV overhead line, 275kV underground cable and 400kV underground cable, 400 kV overhead line, Onshore substation equipment,

Transformers, and Quadrature boosters, described as expansion constants for each of these asset classes

* The £/MW/km expansion costs of each separate sub-sea AC circuit and HVDC circuit
* 132kV overhead circuit capacity and single/double route construction information is used in the calculation of a generator’s local charge.
* Offshore transmission cost and circuit/substation data

1. For a given **Financial Year** "t", the nodal generation TEC figure and generation plant types at each node will be based on the Applicable Value for year "t" in the NETS Seven Year Statement in year "t-1" plus updates to the October of year "t-1". The contracted TECs and generation plant types in the NETS Seven Year Statement include all plant belonging to generators who have a Bilateral Agreement with the TOs. For example, for 2010/11 charges, the nodal generation data is based on the forecast for 2010/11 in the 2009 NETS Seven Year Statement plus any data included in the quarterly updates in October 2009.
2. Scaling factors for different generation plant types are applied on their aggregated capacity for both Peak Security and Year Round backgrounds. The scaling is either Fixed or Variable (depending on the total demand level) in line with the factors used in the Security Standard, for example as shown in the table below.

|  |  |  |
| --- | --- | --- |
| **Generation Plant Type** | **Peak Security Background** | **Year Round Background** |
| Intermittent | Fixed (0%) | Fixed (70%) |
| Nuclear & CCS | Variable | Fixed (85%) |
| Interconnectors | Fixed (0%) | Fixed (100%) |
| Hydro | Variable | Variable |
| Pumped Storage | Variable | Fixed (50%) |
| Peaking | Variable | Fixed (0%) |
| Other (Conventional) | Variable | Variable |

These scaling factors and generation plant types are set out in the Security Standard. These may be reviewed from time to time. The latest version will be used in the calculation of TNUoS tariffs and is published in the Statement of Use of System Charges

1. The Company will categorise plant based on the categorisations described in the Security Standard. Peaking plant will include oil and OCGT technologies and Other (Conv.) represents all remaining conventional plant not explicitly stated elsewhere in the table In the event that a power station is made up of more than one technology type, the type of the higher Transmission Entry Capacity (TEC) would apply.
2. Nodal net demand data for the transport model will be based upon the GSP net demand that Users have forecast to occur at the time of National Grid Peak Average Cold Spell (ACS) Demand for year "t" in the April Seven Year Statement for year "t-1" plus updates to the October of year "t-1".
3. Subject to paragraphs 14.15.15 to 14.15.22, Transmission circuits for **Financial Year** "t" will be defined as those with existing wayleaves for the year "t" with the associated lengths based on the circuit lengths indicated for year "t" in the April NETS Seven Year Statement for year "t-1" plus updates to October of year "t-1". If certain circuit information is not explicitly contained in the NETS Seven Year Statement, The Company will use the best information available.
4. The circuit lengths included in the transport model are solely those, which relate to assets defined as 'Use of System' assets.
5. For HVDC circuits, the impedance will be calculated to provide flows based on a ratio of the capacity provided by the HVDC link relative to the capacities on all major transmission system boundaries that it parallels.

14.15.13 The transport model employs the use of different expansion constants to reflect the difference in costs between (i) AC Circuits and HVDC circuits, (ii) underground and sub-sea circuits, (iii) cabled circuits and overhead line circuits, (iv) 132kV and 275kV circuits, (v) 275kV circuits and 400kV circuits, and (vi) 400kV overhead lines. When calculating the local circuit tariff for a generator, alternative 132kV and offshore expansion constants to those used in the remainder of the tariff calculation are applied to the generator’s local circuits.

1. The circuit expansion constants for HVDC circuits and AC subsea cables are determined on a case by case basis using the costs which are specific to individual projects containing HVDC or AC subsea circuits.

**Adjustments to Model Inputs associated with One-off Works**

1. Where, following the implementation of CUSC Modification CMP203, a User has paid a One-Off Charge that related to One-off Works carried out on an onshore circuit, and such One-off Works would affect the value of a TNUoS tariff paid by the User, the transport model inputs associated with the onshore circuit shall be adjusted by The Company to reflect the asset value that would have been modelled if the works had been undertaken on the basis of the original asset design rather than the One-off Works.
2. Subject to paragraphs 14.15.17 to 14.15.19, where, prior to the implementation of CUSC Modification CMP203, a User has paid a One-Off Charge (or has paid a charge to the relevant TO prior to 1st April 2005 on the same principles as a One-Off Charge) that related to works equivalent to those described under paragraph 14.15.15, an adjustment equivalent to that under paragraph 14.15.15 shall be made to the transport model inputs as follows.
3. Such adjustment shall be made following a User’s request, which must be received by The Company no later than the second occurrence of 31st December following the implementation of CUSC Modification CMP203.
4. The Company shall only make an adjustment to the transport model inputs, under paragraph 14.15.16 where the charge was paid to the relevant TO prior to 1st April 2005 where evidence has been provided by the User that satisfies The Company that works equivalent to those under paragraph 14.15.15 were funded by the User.
5. Where a User has sufficient reason to believe that adjustments under paragraph 14.15.18 should be made in relation to specific assets that affect a TNUoS tariff that applies to one of its sites and outlines its reasoning to The Company, The Company shall (upon the User’s request and subject to the User’s payment of reasonable costs incurred by The Company in doing so) use its reasonable endeavours to assist the User in obtaining any evidence The Company or a TO may have to support its position.
6. Where a request is made under paragraph 14.15.16 on or prior to 31st December in a **Financial Year**, and The Company is satisfied based on the accompanying evidence provided to The Company under paragraph 14.15.17 that it is a valid request, the transport model inputs shall be adjusted accordingly and taken into account in the calculation of TNUoS tariffs effective from the year commencing on the 1st April following this and otherwise from the next subsequent 1st April.
7. The following table provides examples of works for which adjustments to transport model inputs would typically apply:

| **Ref** | **Description of works** | **Adjustments** |
| --- | --- | --- |
| 1 | Undergrounding - A User requests to underground an overhead line at a greater cost. | As the cable cost will be more expensive than the overhead line (OHL) equivalent, the circuit will be modelled as an OHL. |
| 2 | Substation Siting Decision - A User requests to move the existing or a planned substation location to a place that means that the works cannot be justified as economic by the TO. | As the revised substation location may result in circuits being extended. If this is the case, the originally designed circuit lengths (as per the originally designed substation location) would be used in the transport model. |
| 3 | Circuit Routing Decision - A User asks to move an existing or a planned circuit route in a way in which the works cannot be justified as economic by the TO. | As any circuit route changes that extend circuits are likely to result in a greater TNUoS tariff, the originally designed circuit lengths would be used in the transport model. |
| 4 | Building circuits at lower voltages - A User requests lower tower height and therefore a different voltage. | As lower voltage circuits result in a higher expansion constant for this asset class, the circuits would be modelled at the originally designed higher voltage. |

1. The following table provides examples of works for which adjustments to transport model typically would not apply:

| **Ref** | **Description of works** | **Reasoning** |
| --- | --- | --- |
| 1 | Undergrounding - A User chooses to have a cable installed via a tunnel rather than buried. | Cable expansion constants are applied in the transport model regardless of whether a cable is tunnelled and buried, so there is no increased TNUoS cost. |
| 2 | Additional circuit route works - A User asks for screening to be provided around a new or existing circuit route. | Circuit expansion constants are applied in the transport model irrespective of these works, so there is no increased TNUoS cost. |
| 3 | Additional circuit route works - A User requests that a planned overhead line route is built using alternative transmission tower designs. | Circuit expansion constants are applied in the transport model irrespective of these works, so there is no increased TNUoS cost. |
| 4 | Additional substation works - A User asks for screening to be provided around a new or existing substation. | The additional substation works will not affect the User’s TNUoS charge as there is no effect on power flows or circuit costs within the transport model. |
| 5 | Additional substation works - Changes to connection assets (e.g. HV-LV transformers and associated switchgear), metering, additional LV supplies, additional protection equipment, additional building works, etc. | The additional substation works will not affect the User’s TNUoS charge as there is no effect on power flows or circuit costs within the transport model. |
| 6 | Diversion - A User asks to temporarily move an existing or a planned circuit route in a way in which the works cannot be justified as economic by the TO. | The temporary circuit changes will not be incorporated into the transport model. |
| 7 | Connection Entry Capacity (CEC) before Transmission Entry Capacity (TEC). A User asks for a connection in a year prior to the relating TEC; i.e. physical connection without capacity. | No additional works are being undertaken, works are simply being completed well in advance of the generator commissioning. The One-Off Charge reflects the depreciated value of the assets prior to commissioning (and any TNUoS being charged). |
| 8 | Early asset replacement - An asset is replaced prior to the end of its expected life. | As the asset is simply replaced, no data in the transport model is expected to change |
| 9 | Additional Engineering/  Mobilisation costs - A User requests changes to the planned works, that results in additional operational costs. | The data in the transport model is unaffected. |
| 10 | Offshore(Generator Build) - Any of the works described above or under paragraph 14.15.18. | The value of the works will not form part of the asset transfer value therefore will not be used as part of the offshore tariff calculation. |
| 11 | Offshore(Offshore Transmission Owner (OFTO) Build) - Any of the works described above or under paragraph 14.15.18. | As part of determining the TNUoS revenue associated with each asset, the value of the One-Off Works would be excluded when pro-rating the OFTO’s allowed revenue against assets by asset value. |

1. The Company shall publish any adjusted transport model inputs that it intends to use in the calculation of TNUoS tariffs effective from the year commencing on the following 1st April`. Any further adjustments that The Company makes shall be published by The Company upon or before the publication of the final TNUoS tariffs for the year concerned.

### **Model Outputs**

1. The transport model takes the inputs described above and carries out the following steps individually for Peak Security and Year Round backgrounds.
2. Depending on the background, the TEC of the relevant generation plant types are scaled by a percentage as described in 14.15.7, above. The TEC of the remaining generation plant types in each background are uniformly scaled such that total national generation (scaled sum of contracted TECs) equals total national ACS Demand.
3. For each background, the model then uses a DCLF ICRP transport algorithm to derive the resultant pattern of flows based on the network impedance required to meet the nodal net demand using the scaled nodal generation, assuming every circuit has infinite capacity. Flows on individual transmission circuits are compared for both backgrounds and the background giving rise to the highest flow is considered as the triggering criterion for future investment of that circuit for the purposes of the charging methodology. Therefore all circuits will be tagged as Peak Security or Year Round depending upon the background resulting in the highest flow. In the event that both backgrounds result in the same flow, the circuit will be tagged as Peak Security. Then it calculates the resultant total network Peak Security MWkm and Year Round MWkm, using the relevant circuit expansion constants as appropriate.
4. Using these baseline networks for Peak Security and Year Round backgrounds, the model then calculates for a given injection of 1MW of generation at each node, with a corresponding 1MW offtake (net demand) distributed across all demand nodes in the network, the increase or decrease in total MWkm of the whole Peak Security and Year Round networks. The proportion of the 1MW offtake allocated to any given demand node will be based on total background nodal net demand in the model. For example, with a total net GB demand of 60GW in the model, a node with a net demand of 600MW would contain 1% of the offtake i.e. 0.01MW.
5. Given the assumption of a 1MW injection, for simplicity the marginal costs are expressed solely in km. This gives a Peak Security marginal km cost and a Year Round marginal km cost for generation at each node (although not that used to calculate generation tariffs which considers local and wider cost components). The Peak Security and Year Round marginal km costs for demand at each node are equal and opposite to the Peak Security and Year Round nodal marginal km respectively for generation and this is used to calculate demand tariffs. Note the marginal km costs can be positive or negative depending on the impact the injection of 1MW of generation has on the total circuit km.
6. Using a similar methodology as described above in 14.15.27, the local and wider marginal km costs used to determine generation TNUoS tariffs are calculated by injecting 1MW of generation against the node(s) the generator is modelled at and increasing by 1MW the offtake across the distributed reference node. It should be noted that although the wider marginal km costs are calculated for both Peak Security and Year Round backgrounds, the local marginal km costs are calculated on the Year Round background.
7. In addition, any circuits in the model, identified as local assets to a node will have the local circuit expansion constants which are applied in calculating that particular node’s marginal km. Any remaining circuits will have the TO specific wider circuit expansion constants applied.
8. An example is contained in 14.21 Transport Model Example.

## 

## Calculation of local nodal marginal km

1. In order to ensure assets local to generation are charged in a cost reflective manner, a generation local circuit tariff is calculated. The nodal specific charge provides a financial signal reflecting the security and construction of the infrastructure circuits that connect the node to the transmission system.
2. Main Interconnected Transmission System (MITS) nodes are defined as:

* Grid Supply Point connections with 2 or more transmission circuits connecting at the site; or
* connections with more than 4 transmission circuits connecting at the site.

1. Where a Grid Supply Point is defined as a point of supply from the National Electricity Transmission System to network operators or non-embedded customers excluding generator or interconnector load alone. For the avoidance of doubt, generator or interconnector load would be subject to the circuit component of its Local Charge. A transmission circuit is part of the National Electricity Transmission System between two or more circuit-breakers which includes transformers, cables and overhead lines but excludes busbars and generation circuits.
2. Generators directly connected to a MITS node will have a zero local circuit tariff.
3. Generators not connected to a MITS node will have a local circuit tariff derived from the local nodal marginal km for the generation node i.e. the increase or decrease in marginal km along the transmission circuits connecting it to all adjacent MITS nodes (local assets).

## Calculation of zonal marginal km

1. Given the requirement for relatively stable cost messages through the ICRP methodology and administrative simplicity, nodes are assigned to zones. The currently applicable number of generation zones is detailed in **The Company's Statement of Use of System Charges** which is available from the **Charging website.**
2. Demand zone boundaries have been fixed and relate to the GSP Groups used for energy market settlement purposes.
3. The nodal marginal km are amalgamated into zones by weighting them by their relevant generation or demand capacity.
4. Generators will have zonal tariffs derived from both, the wider Peak Security nodal marginal km; and the wider Year Round nodal marginal km for the generation node calculated as the increase or decrease in marginal km along all transmission circuits except those classified as local assets.

The zonal Peak Security marginal km for generation is calculated as:





Where

Gi = Generation zone

j = Node

NMkmPS = Peak Security Wider nodal marginal km from transport model

WNMkmPS = Peak Security Weighted nodal marginal km

ZMkmPS = Peak Security Zonal Marginal km

Gen = Nodal Generation (scaled by the appropriate Peak Security Scaling factor) from the transport model

Similarly, the zonal Year Round marginal km for generation is calculated as





Where

NMkmYR = Year Round Wider nodal marginal km from transport model

WNMkmYR = Year Round Weighted nodal marginal km

ZMkmYR = Year Round Zonal Marginal km

Gen = Nodal Generation (scaled by the appropriate Year Round Scaling factor) from the transport model

1. The zonal Peak Security marginal km for demand zones are calculated as follows. If Nodal Demand from a node is less than 0 (Exporting) the nodal demand will be set to zero and therefore not contribute to the Zonal marginal km





Where:

Di = Demand zone

Dem = Positive Nodal Net Demand from transport model

Similarly, the zonal Year Round marginal km for demand zones are calculated as follows:





1. The number of generation zones will be fixed to 27 zones and the assignment of existing relevant nodes to these 27 generation zones will be fixed to those that are effective as of 31st March 2021 based on methodology in effect during the 2020/21. Relevant nodes are considered to be those with generation connected to them. **Financial Year**. Any newly created relevant nodes will be assigned to one of the 27 generation zones.
2. Not Used
3. Not Used
4. Not Used

**Accounting for Sharing of Transmission by Generators**

1. A proportion of the marginal km costs for generation are shared incremental km reflecting the ability of differing generation technologies to share transmission investment. This is reflected in charges through the splitting of Year Round marginal km costs for generation into Year Round Shared marginal km costs and Year Round Not-Shared marginal km which are then used in the calculation of the wider £/kW generation tariff.
2. The sharing between different generation types is accounted for by (a) using transmission network boundaries between generation zones set by connectivity between generation charging zones, and (b) the proportion of Low Carbon and Carbon generation behind these boundaries.
3. The zonal incremental km for each generation charging zone is split into each boundary component by considering the difference between it and the neighbouring generation charging zone using the formula below;



Where;

BIkmab = boundary incremental km between generation charging zone A and generation charging zone B

ZIkm = generation charging zone incremental km.

1. The table below shows the categorisation of Low Carbon and Carbon generation. This table will be updated by The Company in the Statement of Use of System Charges as new generation technologies are developed.

|  |  |
| --- | --- |
| **Carbon** | **Low Carbon** |
| Coal | Wind |
| Gas | Hydro (excl. Pumped Storage) |
| Biomass | Nuclear |
| Oil | Marine |
| Pumped Storage | Tidal |
| Interconnectors |  |

Determination of Connectivity

1. Connectivity is based on the existence of electrical circuits between TNUoS generation charging zones that are represented in the Transport model. Where such paths exist, generation charging zones will be effectively linked via an incremental km transmission boundary length. These paths will be simplified through in the case of;

* Parallel paths – the longest path will be taken. An illustrative example is shown below with x, y and z representing the incremental km between zones.



* Parallel zones – parallel zones will be amalgamated with the incremental km immediately beyond the amalgamated zones being the greater of those existing prior to the amalgamation. An illustrative example is shown below with a, b, c, and d representing the initial incremental km between zones, and x and y representing the final incremental km following zonal amalgamation.



1. An illustrative Connectivity diagram is shown below:



The arrows connecting generation charging zones and amalgamated generation charging zones represent the incremental km transmission boundary lengths towards the notional centre of the system. Generation located in charging zones behind arrows is considered to share based on the ratio of Low Carbon to Carbon cumulative generation TEC within those zones.

1. The Company will review Connectivity at the beginning of a new price control period, and under exceptional circumstances such as major system reconfigurations. If any such reassessment is required, it will be undertaken against a background of minimal change to existing Connectivity and in line with the notification process set out in the Transmission Licence and the CUSC.

Calculation of Boundary Sharing Factors

1. Boundary sharing factors (BSFs) are derived from the comparison of the cumulative proportion of Low Carbon and Carbon generation TEC behind each of the incremental MWkm boundary lengths using the following formulae –

If , then all Year round marginal km costs are shared i.e. the BSF is 100%.

Where:

LC = Cumulative Low Carbon generation TEC behind the relevant transmission boundary

C = Cumulative Carbon generation TEC behind the relevant transmission boundary

If  then the BSF is calculated using the following formula: -



Where:

BSF = boundary sharing factor.

1. The shared incremental km for each boundary are derived from the multiplication of the boundary sharing factor by the incremental km for that boundary;



Where;

SBIkmab = shared boundary incremental km between generation charging zone A and generation charging zone B

BSFab = generation charging zone boundary sharing factor.

1. The shared incremental km is discounted from the incremental km for that boundary to establish the not-shared boundary incremental km. The not-shared boundary incremental km reflects the cost of transmission investment on that boundary accounting for the sharing of power stations behind that boundary.



Where;

NSBIkmab = not shared boundary incremental km between generation charging zone A and generation charging zone B.

1. The shared incremental km for a generation charging zone is the sum of the appropriate shared boundary incremental km for that generation charging zone as derived from the connectivity diagram.



Where;

ZMkmnYRS = Year Round Shared Zonal Marginal km for generation charging zone n.

1. The not-shared incremental km for a generation charging zone is the sum of the appropriate not-shared boundary incremental km for that generation charging zone as derived from the connectivity diagram.



Where;

ZMkmnYRNS = Year Round Not-Shared Zonal Marginal km for generation zone n.

## Deriving the Final Local £/kW Tariff and the Wider £/kW Tariff

1. The zonal marginal km (ZMkmGi) are converted into costs and hence a tariff by multiplying by the **Expansion Constant** and the **Locational Security Factor** (see below). The nodal local marginal km (NLMkmL) are converted into costs and hence a tariff by multiplying by the **Expansion Constant** and a **Local Security Factor**.

### 

### **The Expansion Constant**

1. The expansion constant is calculated for a number of asset classes. It is expressed in £/MW/km, and represents the annuitised value of the transmission infrastructure capital investment required to transport 1 MW over 1 km. Its magnitude is derived from the projected cost, expressed as £/MW/km, of new or reinforced circuit capacity, including an estimate of the cost of capital, to provide for future system expansion. This cost may be derived from the cost of a new line, or from reinforcements, where a reinforcement is an investment that adds to the capacity or life of an existing line, taking account of the years for which the new capacity will apply, the capacity added, and the length. Reinforcements to existing circuits that add neither life nor capacity, will be ignored. For reinforcements, account is taken of the remaining asset life prior to the investment, and of the new remaining asset life after the investment. For any investment for which the **Onshore Transmission** **Licensee** is unable to give **The Company** the remaining life before the investment was made, a default assumption of 0 years of remaining life will be applied. For any investment for which the **Onshore Transmission** **Licensee** is unable to give **The Company** the remaining life after the investment was made, a default assumption of 45 years of remaining life will be applied.
2. In the methodology, the expansion constant is used to convert the marginal km figure derived from the transport model into a £/MW signal. The tariff model performs this calculation, in accordance with 14.15.95 – 14.15.117, and also then calculates the residual element of the overall tariff (to ensure correct revenue recovery in accordance with the price control), in accordance with 14.15.133.
3. For each circuit type (line or cable) and voltage (each “asset type”) used onshore, an individual calculation is carried out to establish a £/MW/km figure, these provide the basis of the onshore circuit expansion constants for each asset type discussed in 14.15.73 – 14.15.87. In order to simplify the calculation a unity power factor is assumed, converting £/MVA/km to £/MW/km. This reflects the fact that tariffs and charges are based on real power.
4. For each asset class k, in the first year of the date of implementation of CMP315, 10 years’ worth of historic data on each new investment from the **Onshore Transmission Licensees** is to be used to perform the calculation in 14.15.64 and thereby populate inputECnewk in 14.15.65 These data are to each have the appropriate number of years of inflation applied to bring each value up to the current year at the time this calculation is carried out.The inflation to be used is TOPI, (as defined in the Onshore Transmission Licensees’ Transmission Licences)
5. In each subsequent year, one year’s worth of new data on new investments from the **Onshore Transmission Licensees** relating to any new assets in class k, is used to perform the calculation in 14.15.64 and thereby populate inputECnewk in 14.15.65. This cost data first has one year’s inflation applied to bring its value up to the current year at the time this calculation is carried out. The inflation to be used is TOPI, (as defined in the Onshore Transmission Licensees’ Transmission Licences)
6. The onshore £/MW/km data for each asset class, for example the data for the 400 kV overhead line asset class which comprises the 400 kV line expansion constant, is calculated as follows :

For each relevant new circuit, , or circuit reinforcement for which the TO has provided data over the relevant period as specified in 14.15.62 and 14.15.63 , the following calculation is performed :

* 1. Where a reinforcement to an existing circuit results in both an increase in the capacity of the circuit and the expected life of that circuit, the cost of the investment is allocated across each of these outcomes in the following manner:
     1. The cost allocated to the marginal increase in circuit capacity (MW) is calculated as:

1. The cost allocated to the marginal increase in circuit life (years) is calculated as:

Where;

and

Where:

The “estimated life of circuit from investment completion” refers to the number of years between the relevant investment having been completed and the expected new end of life of the asset following the investment.

The “estimated increase in the life of circuit” refers to the marginal increase in the expected life of the circuit which has resulted as a consequence of the investment having been made.

* 1. The £/MW/km cost of each investment (or each part of the investment allocated under subparagraph a. above) is calculated as follows :

Where Relevant MW has the following values:

* + 1. Where the investment cost relates to a new circuit or to an increase in life of an existing circuit (except when part of the cost is allocated under sub paragraph a. above), the Relevant MW will be the rating of that circuit.
    2. Where the investment cost relates to an increase in capacity of an existing circuit (or part of the cost allocated as such under sub-paragraph a. above), the Relevant MWs refers to the new MW capacity of the circuit minus the previous MW capacity of the circuit prior to the investment. That is, it represents the marginal increase in capacity provided for by the investment.
    3. Where the investment cost relates to an increase in the life of the asset allocated as such under sub-paragraph a. above, the Relevant MW refers to the previous MW capacity of the circuit prior to the relevant investment having taken place.
  1. The £/MW/km cost is then converted into an annual figure by multiplying it by an annuity factor. The formula used to calculate the annuity factor is shown below:

The Weighted Average Cost of Capital (WACC) used in the calculation of the annuity factor here is that which is established at the start of each price control for **NGET**. It remains constant throughout a price control period. The WACC to be used is **NGET**'s value, taken as a representative value for all licensees.

Where AssetLife has the following values:

* + 1. Where the investment cost relates to a new circuit, AssetLife refers to the expected life of the circuit in years from the date the investment is completed.
    2. Where the investment cost relates to an increase in life of an existing circuit (or part of the cost allocated as such under sub-paragraph a. above), AssetLife refers to the marginal increase in the expected life of the circuit which has resulted as a consequence of the investment having been made.
    3. Where the investment cost relates to an increase in the MW capacity of the asset (or part of the cost allocated as such under sub-paragraph a. above), AssetLife refers to the expected life of the circuit in years from the date the investment is completed.
  1. The £/MW/km costs for all assets (or where relevant, the costs for portions of assets allocated under sub-paragraph a. above) within a particular asset class are then weighted by the product of Relevant MW (as calculated under sub-paragraph b. above), km (“circuit length in km” as used in sub-paragraph b. above) and years of life (AssetLife used in sub-paragraph c. above), so that a MWkmyears weighted average £/MW/km value for that asset class is calculated

1. The weighted average £/MW/km value for each asset class is multiplied by an overhead factor which is derived as in 14.15.66. The resulting value is the input Expansion Constant datum for asset class k (inputECnewk)
2. The overhead factor is used to add a share of the annual transmission overheads (maintenance, rates etc). It represents the total business overhead in any year divided by the total Gross Asset Value (GAV) of the transmission system. This is recalculated at the start of each price control period. The currently applicable overhead factor used in the calculation of the current expansion constant is detailed in The Company's **Statement of Use of System Charges** which is available from the charging details to be found on **The Company Website**.

.

1. A compound circuit is made up of all the chargeable elements it contains (overhead lines, underground cables, transformers and quad boosters) plus any substation bays used exclusively by that circuit plus a share of any substation bays not directly connected to any circuit. For example if a double bus substation had four circuits and a single bus coupler it would contribute 1¼ bays to the compound circuit.

The circuit length of the non-circuit elements will be based on the average for that voltage level of the data submitted by the Transmission Owners.

1. The above steps are also taken for each other asset class including lines and cables at other voltages, transformers, and switchgear bays
2. The new datum input ECnewk k for asset class k is given a weighting of 13%, and the last year’s datum ECy-1k for that asset class has one year’s inflation applied and is given a weighting of 87%. This gives the actual EC for year y for asset class k, thus : pre-annualisedECyk = ECnewk \*0.13 + ECy-1 \* inflation \* 0.87. The inflation used is **TOPI**, (May–October average increase, as defined in the **Onshore Transmission** **Licensees‘ Transmission Licences**)

.

1. This process is carried out for each voltage asset class onshore, along with other adjustments to take account of upgrade options, see 14.15.73
2. For each voltage (400kV, 275kV and 132 kV) the asset classes are:
   1. Overhead line
   2. Underground cable
   3. Substation bay
   4. Quadrature booster
   5. Transformers to other transmission voltages
3. The current set of expansion constants for each asset class are detailed in **The Company's Statement of Use of System Charges** which is available from the **Charging website**.

14.15..

1. The 132kV onshore circuit expansion constant is applied on a TO basis. This is to reflect the regional variation of plans to rebuild circuits at a lower voltage capacity to 400kV. The 132kV cable and line expansion constants are calculated on the proportion of 132kV circuits likely to be uprated to 400kV. The 132kV expansion constantsare then calculated by weighting the 132kV cable and overhead line costs, based on the proportion of 132kV circuitry to be uprated to 400kV on average within a price control period as identified from **The Company**’s own network planning exercise. For example, in the TO areas of **NGET** and Scottish Power where there are no plans to uprate any 132kV circuits, the full cable and overhead line costs of a 132kV circuit are reflected in the 132kV expansion constant calculation.

1. The 275kV onshore circuit expansion constantis applied on a GB basis and includes a weighting of 83%, or such updated figure as the ESO identify from its own network planning exercises, of the relevant 400kV cable and overhead line factor. This is to reflect the averaged proportion of circuits across all three **Onshore Transmission Licensees** which are likely to be uprated from 275kV to 400kV across GB within a price control period.

.

1. AC sub-sea cable and HVDC circuit expansion constantsare calculated on a case by case basis using actual project costs (Specific Circuit Expansion Constants).
2. Calculation of HVDC circuit expansion constants, and AC sub-sea circuit expansion constants, shall include only: the cost of the converters (where applicable); and the cost of the cable; and a percentage of the total overhead project costs, defined as the combined costs of the cables and converters (as relevant) divided by the total capital cost of the project
3. The TO specific onshore circuit expansion constantswhich are currently applicable, are detailed in The Company's **Statement of Use of System Charges** which is available from the **Charging website**.

**Onshore Local Circuit expansion constants**

1. The local onshore circuit tariff is calculated using local onshore circuit expansion constants. These expansion constantsare calculated using the same methodology as the onshore wider 400 kV expansion constantbut without taking into account the proportion of circuit kms that are planned to be uprated.
2. In addition, the 132kV onshore overhead line circuit expansion constantis sub divided into four more specific expansion constants. This is based upon maximum (winter) circuit continuous rating (MVA) and route construction whether double or single circuit. The 132kV onshore overhead line circuit expansion constantswhich are currently applicable, are detailed in **The Company's Statement of Use of System Charges** which is available from the **Charging website**.

### 

### **Offshore Circuit expansion constants**

1. Offshore expansion constants (£/MWkm) are derived from information provided by Offshore Transmission Owners for each offshore circuit. Offshore expansion constantsare Offshore Transmission Owner and circuit specific. Each Offshore Transmission Owner will periodically provide, via the STC, information to derive an annual circuit revenue requirement. The offshore circuit revenue shall include revenues associated with the Offshore Transmission Owner’s reactive compensation equipment, harmonic filtering equipment, asset spares and HVDC converter stations.
2. In the year that the offshore transmission assets are transferred to the Offshore Transmission Owner , the offshore circuit expansion constantwould be calculated as follows:

Where:

CRevOFTO1 = The offshore circuit revenue in £ for Year 1

L = The total circuit length in km of the offshore circuit

CircRat = The continuous rating of the offshore circuit

1. In all subsequent years, the offshore expansion constantwould be calculated as follows:

Where:

AvCRevOFTO = The annual offshore circuit revenue averaged over the remaining years of the onshore National Electricity Transmission System Operator (NETSO) price control

L = The total circuit length in km of the offshore circuit

CircRat = The continuous rating of the offshore circuit

1. For the avoidance of doubt, the offshore circuit revenue values, *CRevOFTO1* and *AvCRevOFTO* shall be determined using asset values after the removal of any One-Off Charges.
2. Prevailing **Offshore Transmission Owner** specific expansion constants will be published in **The Company's Statement of Use of System Charges** which is available from the Charging part of **The Company’s Website**. These shall be recalculated for the start of each price control period using the formula in paragraph 14.15.82. For each subsequent year within the price control period, these expansion constants will be adjusted by the annual Offshore Transmission Owner specific indexation factor, *OFTOInd*, calculated as follows;

`



where:

*OFTOIndt,f* = the indexation factor for Offshore Transmission

Owner *f* in respect of **Financial Year** *t*;

*OFTORevIndt,f* = the indexation rate applied to the revenue of

Offshore Transmission Owner *f* under the terms of its transmission licence in respect of **Financial Year** *t*; and

*TOPIt* = the indexation rate applied to the expansion

constant in respect of **Financial Year** *t*.

**Offshore Interlinks**

14.15.87 The revenue associated with an Offshore Interlink shall be divided entirely between those generators benefiting from the installation of that Offshore Interlink. Each of these Users will be responsible for their charge from their charging date, meaning that a proportion of the Offshore Interlink revenue may be socialised prior to all relevant Users being chargeable. The proportion associated with each User will be based on the Measure of Capacity to the MITS using the Offshore Interlink(s) in the event of a single circuit fault on the User’s circuit from their offshore substation towards the shore, compared to the Measure of Capacity of the other Users.

Where:

An *Offshore Interlink* is a circuit which connects two offshore substations that are connected to a Single Common Substation. It is held in open standby until there is a transmission fault that limits the User’s ability to export power to the Single Common Substation. In the Transport Model, they are to be modelled in open standby.

A *Single Common Substation* is a substation where:

i. each substation that is connected by an Offshore Interlink is connected via at least one circuit without passing through another substation; and

ii. all routes connecting each substation that is connected by an Offshore Interlink to the MITS pass through.

The Measure of Capacity to the MITS for each Offshore substation is the result of the following formula or zero whichever is larger. For the situation with only one interlink, all terms relating to C should be set to zero:

For Substation A:

min { CapIAB, ILFA × TECA - RCapA, CapB - ILFB × TECB + min (CapIBC, CapC - ILFC × TECC) }

For Substation B:

min { ILFB × TECB - RCapB, min (CapIAB, CapA - ILFA × TECA )

+ min ( CapIBC, CapC - ILFC × TECC) }

For Substation C:

min { CapIBC, ILFC × TECC - - RCapC, CapB - ILFB × TECB + min (CapIAB, CapA – ILFA × TECA) }

and

CapIAB = total capacity of the Offshore Interlink between substations A and B

CapIBC = total capacity of the Offshore Interlink between substations B and C

CapX = total capacity of the circuit between offshore substation X and the Single Common Substation, where X is A, B or C.

RCapX = remaining capacity of the circuit between offshore substation X and the Single Common Substation in the event of a single cable fault, where X is A, B or C.

TECX = the sum of the TEC for the Users connected, or contracted to connect, to offshore substation X, where X is A, B or C, where the value of TEC will be the maximum TEC that each User has held since the initial charging date, or is contracted to hold if prior to the initial charging date.

ILFX = Offshore Interlink Load Factor, where X is A, B or C.

The Offshore Interlink Load Factor (ILF) is based on the Annual Load Factor (ALF). Until all the Users connected to a Single Common Substation have a station specific Annual Load Factor based on five years of data, the generic ALF for the fuel type will be used as the ILF for all stations. When all Users have a station specific ALF, the value of the ALF in the first such year will be used as the ILF in the calculation for all subsequent **Financial Years**.

14.15.88 The apportionment of revenue associated with Offshore Interlink(s) in 14.15.85 applies in situations where the Offshore Interlink was included in the design phase, or if one or more User(s) has already financially committed or been commissioned then only where that User(s) agrees to the Offshore Interlink.

14.15.89 Alternatively to the formula specified in 14.15.85 the proportion of the OFTO revenue associated with the Offshore Interlink allocated to each generator benefiting from the installation of an Offshore Interlink may be agreed between these Users. In this event:

a. All relevant Users shall notify The Company of its respective proportions three months prior the OTSDUW asset transfer in the case of a generator build, or the charging date of the first generator, in the case of an OFTO build.

b. All relevant Users may agree to vary the proportions notified under (a) by each writing to The Company three months prior to the charges being set for a given **Financial Year**.

c. Once a set of proportions of the OFTO revenue associated with the Offshore Interlink has been provided to The Company, these will apply for the next and future **Financial Years** unless and until The Company is informed otherwise in accordance with (b) by all of the relevant Users.

d. If all relevant Users are unable to reach agreement on the proportioning of the OFTO revenue associated with the Offshore Interlink they can raise a dispute. Any dispute between two or more Users as to the proportioning of such revenue shall be managed in accordance with CUSC Section 7 Paragraph 7.4.1 but the reference to the ‘Electricity Arbitration Association’ shall instead be to the ‘Authority’ and the Authority’s determination of such dispute shall, without prejudice to apply for judicial review of any determination, be final and binding on the Users.

### **The Locational Onshore Security Factor**

1. The locational onshore security factor for everything other than Identified Onshore Circuits is derived by running a secure DCLF ICRP transport study of the network excluding local circuits and Identified Onshore Circuits based on the same market background as used for Zoning in the DCLF ICRP transport model. This calculates the nodal marginal costs where peak net demand can be met despite the Security and Quality of Supply Standard contingencies (simulating single and double circuit faults) on the network. Essentially the calculation of secured nodal marginal costs is identical to the process outlined above except that the secure DCLF study additionally calculates a nodal marginal cost taking into account the requirement to be secure against a set of worse case contingencies in terms of maximum flow for each circuit.
2. For the purposes of 14.15.88 the secured nodal cost differential is compared to that produced by the DCLF ICRP transport model and the resultant ratio of the two determines the locational security factor using the Least Squares Fit method. Further information may be obtained from the charging website[[1]](#footnote-2).
3. For the purposes of 14.15.88 the locational onshore security factor, derived in accordance with paragraphs 14.15.88 and 14.15.89 and expressed to two decimal places, is based on an average from a number of studies conducted by The Company to account for future network developments. This security factor is reviewed for each price control period and fixed for the duration. The locational onshore security factor which is currently applicable, is detailed in The Company's **Statement of Use of System Charges**, which is available from the **Charging website.**

14.15.92A An Identified Onshore Circuit shall be defined as a single transmission HVDC subsea circuit or a single transmission AC subsea circuit between two MITS Nodes where there is only one route for the power to flow between the two MITS Nodes. The expansion constants for Identified Onshore Circuits are adjusted by the locational onshore security factor calculated in 14.15.90. When the locational onshore security factor is applied as per Section 14.15.96 and 14.15.97, this would result in an effective locational onshore security factor for Identified Onshore Circuits of 1.0.

### 

**Local Security Factors**

1. Local onshore security factors are generator specific and are applied to a generator’s local onshore circuits. If the loss of any one of the local circuits prevents the export of power from the generator to the MITS then a local security factor of 1.0 is applied. For generation with circuit redundancy, a local security factor is applied that is equal to the locational security factor, derived in accordance with paragraphs 14.15.88 and 14.15.90.
2. Where a Transmission Owner has designed a local onshore circuit (or otherwise that circuit once built) to a capacity lower than the aggregated TEC of the generation using that circuit, then the local security factor of 1.0 will be multiplied by a Counter Correlation Factor (CCF) as described in the formula below;



Where; Dmin = minimum annual net demand (MW) supplied via that circuit in the absence of that generation using the circuit

Tcap = transmission capacity built (MVA)

Gcap = aggregated TEC of generation using that circuit

CCF cannot be greater than 1.0.

1. A specific offshore local security factor (LocalSF) will be calculated for each offshore connection using the following methodology:



Where:

NetworkExportCapacity = the total export capacity of the network disregarding any Offshore Interlinks

k = the generation connected to the offshore network

1. The local offshore security factor for single circuits with a single cable will be 1.0 and for multiple circuit connections will be capped at the locational onshore security factor, derived in accordance with 14.15.88-14.15.90.

14.15.98 The offshore local security factor for configurations with one or more Offshore Interlinks is updated so that the offshore circuit tariff will include the proportion of revenue associated with the Offshore Interlink(s). The specific offshore local security factor for configurations involving an Offshore Interlink, which may be greater than the locational onshore security factor, will be calculated for each offshore connection using the following methodology:



Where:

IRevOFTO = The appropriate proportion of the Offshore Interlink(s) revenue in £ associated with the offshore connection calculated in 14.15.85

CRevOFTO = The offshore circuit revenue in £ associated with the circuit(s) from the offshore substation to the Single Common Substation.

LocalSFinitial = Initial Local Security Factor calculated in 14.15.93 and 14.15.94

And other definitions as in 14.15.93.

### **Initial Transport Tariff**

1. First an Initial Transport Tariff (ITT) must be calculated for both Peak Security and Year Round backgrounds. For Generation, the Peak Security zonal marginal km (ZMkmPS), Year Round Not-Shared zonal marginal km (ZMkmYRNS) and Year Round Shared zonal marginal km (ZMkmYRS) are simply multiplied by the expansion constant and the locational security factor to give the Peak Security ITT, Year Round Not-Shared ITT and Year Round Shared ITT respectively:







Where

ZMkmGiPS = Peak Security Zonal Marginal km for each generation zone ZMkmGiYRNS = Year Round Not-Shared Zonal Marginal km for each generation charging zone

ZMkmGiYRS = Year Round Shared Zonal Marginal km for each generation charging zone

EC = Expansion Constant

LSF = Locational Security Factor

ITTGiPS  = Peak Security Initial Transport Tariff (£/MW) for each generation zone

ITTGiYRNS = Year Round Not-Shared Initial Transport Tariff (£/MW) for each generation charging zone

ITTGiYRS = Year Round Shared Initial Transport Tariff (£/MW) for each generation charging zone.

1. Similarly, for demand the Peak Security zonal marginal km ( ZMkmPS) and Year Round zonal marginal km (ZMkmYR) are simply multiplied by the expansion constant and the locational security factor to give the Peak Security ITT and Year Round ITT respectively:





Where

ZMkmDiPS = Peak Security Zonal Marginal km for each demand zone

ZMkmDiYR = Year Round Zonal Marginal km for each demand zone

ITTDiPS = Peak Security Initial Transport Tariff (£/MW) for each demand one

ITTDiYR = Year Round Initial Transport Tariff (£/MW) for each demand zone

1. The next step is to multiply these ITTs by the expected metered triad gross GSP group demand and generation capacity to gain an estimate of the initial revenue recovery for both Peak Security and Year Round backgrounds. The metered triad gross GSP group demand and generation capacity are based on analysis of forecasts provided by Users and are confidential.

Metered triad gross GSP group demand is net demand for all GSP groups less embedded exports for all GSP groups.

Where

ITRRG = Initial Transport Revenue Recovery for generation

GGi = Total forecast Generation for each generation zone (based

on analysis of confidential User forecasts)

ITRRD = Initial Transport Revenue Recovery for gross GSP group

demand

DDi = Total forecast Metered Triad gross GSP group Demand for

each demand zone (based on analysis of confidential User forecasts)

In addition, the initial tariffs for generation are also multiplied by the **Peak Security flag** when calculating the initial revenue recovery component for the Peak Security background. When calculating the initial revenue recovery for the Shared component of the Year Round background, the initial tariffs are multiplied by the **Annual Load Factor** (see below). When calculating the initial revenue recovery for the Not Shared component of the Year Round background, the initial tariffs are multiplied by the **Year Round Not Shared Flag**.

**Peak Security (PS) Flag**

1. The revenue from a specific generator due to the Peak Security locational tariff needs to be multiplied by the appropriate Peak Security (PS) flag. The PS flags indicate the extent to which a generation plant type contributes to the need for transmission network investment at peak demand conditions. The PS flag is derived from the contribution of differing generation sources to the demand security criterion as described in the Security Standard. In the event of a significant change to the demand security assumptions in the Security Standard, National Grid will review the use of the PS flag.

|  |  |
| --- | --- |
| Generation Plant Type | PS flag |
| Intermittent | 0 |
| Other | 1 |

**Year Round Not Shared (YRNS) Flag**

1. The revenue from a specific generator due to the Year Round Not Shared locational tariff needs to be multiplied by the appropriate Year Round Not Shared (YRNS) flag. The YRNS flag indicates the extent to which a generation plant type contributes to the need for transmission network investment at year round demand conditions in areas of the System where the proportion of Low Carbon generation exceeds Carbon generation as defined in 14.15.49.

|  |  |
| --- | --- |
| Generation Plant Type | YRNS flag |
| Non Conventional Carbon | 1 |
| Conventional Carbon | ALF |

**Annual Load Factor (ALF)**

1. The ALF for each individual Power Station is calculated using the relevant TEC (MW) and corresponding output data. Where output data is not available for a Power Station, including for new Power Stations and emerging Power Station technologies, generic data for the appropriate generation plant type will be used.

1. For a given **Financial Year** “t” the Power Station ALF will be based on information from the previous five **Financial Years**, calculated for each **Financial Year** as set out below.



Where:

GMWhp is the maximum of FPN or actual metered output in a Settlement Period related to the power station TEC (MW); and

TECp is the TEC (MW) applicable to that Power Station for that Settlement Period including any STTEC and LDTEC, accounting for any trading of TEC.

1. The appropriate output (FPN or actual metered) figure is derived from **BM Unit** data available to The Company and relates to the total TEC of the Power Station.
2. Once all five **Financial Year** ALFs have been calculated for the individual Power Station they are compared, and the highest and lowest figures are discarded. The final ALF, to be used for transmission charging purposes, is calculated as the average of the remaining three ALFs.
3. In the event that only four **Financial Years** of complete output (FPN or actual metered) data are available for an individual Power Station then the higher three **Financial Years** ALF would be used in the calculation of the final ALF. In the event that only three **Financial Years** of complete output (FPN or actual metered) data are available then these three **Financial Years** would be used.
4. Due to the aggregation of output (FPN or actual metered) data for dispersed generation (e.g. cascade hydro schemes), where a single generator BMU consists of geographically separated power stations, the ALF would be calculated based on the total output of the BMU and the overall TEC of those Power Stations.
5. In the event that there are not three full **Financial Years** of an individual power station’s output available, missing output (FPN or actual metered) data would be replaced by generic data for that generation plant type to ensure three **Financial Years** of information are available for the Power Station. The derivation of the generic data is described in paragraphs 14.15.111-14.15.114.
6. Users will receive draft ALFs before 25th December of the **Financial Year** (t-1) for the **Financial Year** (t) and will have a period of 15 **Business Days**
7. from date of publishing to notify the Company of any errors. Failure to agree changes relating to errors will be treated as a charging dispute under the CUSC.
8. The ALFs used in the setting of final tariffs will be published in the annual Statement of Use of System Charges. Changes to ALFs after this publication will not result in changes to published tariffs (e.g. following dispute resolution).

**Derivation of Generic ALFs**

1. The generic ALF is derived from the average annual output of the ten most recently commissioned GB generation of a particular generation plant type that have at least five **Financial Years**’ data, using an identical methodology to that used for the Power Station specific calculation described above. Where less than ten GB generators of a particular generation plant type exist, then data from all existing generators of that particular generation plant type will be used. Example generation plant type categories are listed below;

|  |
| --- |
| **Fuel Type** |
| Biomass |
| Coal |
| Gas |
| Hydro |
| Nuclear (by reactor type) |
| Oil & OCGTs |
| Pumped Storage |
| Onshore Wind |
| Offshore Wind |
| CHP |

1. The Company will keep these categories under review and update as necessary. Where within a category there is a significant locational difference consideration will be given to zonal generic factors. The factors used will be published in the Statement of Use of System Charges and will be reviewed annually.
2. If a User can demonstrate that the generation plant type of a Power Station has changed, consideration will be given to the use of relevant generic ALF information in the calculation of their charges until sufficient specific data is available.
3. For new and emerging generation plant types, where insufficient data is available to allow a generic ALF to be developed, The Company will use the best information available e.g. from manufacturers and data from use of similar technologies outside GB. The factor will be agreed with the relevant Generator. In the event of a disagreement the standard provisions for dispute in the CUSC will apply.

### **TNUoS Embedded Export Tariff**

1. Embedded exports are exports measured on a half-hourly basis by Metering Systems, in accordance with the BSC, that are not subject to generation TNUoS.
2. The embedded export tariff will be applied to the metered Triad volumes of Embedded Exports for each demand zone as follows:

Where

ITTDiPS = Peak Security Initial Transport Tariff for the demand zone;

ITTDiYR = Year Round Initial Transport Tariff for the demand zone, and

EX:

First **Financial Year** following the implementation date of CMP 264/265:

Second **Financial Year** following the implementation date of CMP 264/265:

Third **Financial Year** following the implementation date of CMP 264/265 and every subsequent **Financial Year**:

*=* *AGIC*

Where

XP = Value of demand residual in **Financial Year** prior to implementation

AGIC = The Avoided GSP Infrastructure Credit (AGIC) which represents the unit   
cost of infrastructure reinforcement at GSPs which is avoided as a consequence of embedded generation connected to the distribution networks served by those GSPs. It is calculated from the average annuitised cost of that infrastructure reinforcement divided by the average capacity delivered by a supergrid transformer.

The Avoided GSP Infrastructure Credit is calculated at the beginning of each price control period and in the first applicable **Financial Year** following the implementation date of CMP264/265 using data submitted by onshore TSOs as part of the price control process. The data used is from the most recent [20] schemes submitted under the price control process and indexed each year by the TOPI formula set out in 14.3.6 until the end of the price control. For the avoidance of doubt, this approach does not include the cost of the supergrid transformers or any other connection assets as they are paid for by the relevant DNOs thorough their connection charges.

The Value of EETDi will be floored at zero, so that EETDi is always zero or positive.

### **Initial Revenue Recovery**

### For the Peak Security background the initial tariff for generation is multiplied by the total forecast generation capacity and the PS flag to give the initial revenue recovery:



Where

ITRRGPS = Peak Security Initial Transport Revenue Recovery for generation

GGi = Total forecast Generation for each generation zone (based on analysis of confidential User forecasts)

FPS = Peak Security flag appropriate to that generator type

n = Number of generation zones

The initial revenue recovery for gross GSP group demand for the Peak Security background is calculated by multiplying the initial tariff by the total forecast metered triad gross GSP group demand:



Where:

ITRRDPS = Peak Security Initial Transport Revenue Recovery for gross GSP

group demand

DDi = Total forecast Metered Triad gross GSP group Demand for each demand zone (based on analysis of confidential User forecasts)

### For the Year Round background, the initial tariff for generation is multiplied by the total forecast generation capacity whilst calculating Initial Recovery for the Not-Shared component from Non Conventional Carbon. For Conventional Carbon the initial tariff for the Not Shared component is multiplied by both, the total forecast generation capacity and the ALF to give the initial revenue recovery. The initial tariff for the Shared component is multiplied by both, the total forecast generation capacity and the ALF to give the initial revenue recovery:



Where:

ITRRGYRNSNCC = Year Round Not-Shared Initial Transport Revenue Recovery for

Non Conventional Carbon generation

ITRRGYRNSCC = Year Round Not-Shared Initial Transport Revenue Recovery for

Conventional Carbon generation

ITRRGYRNS = Year Round Not-Shared Initial Transport Revenue Recovery for

generation

ITRRGYRS = Year Round Shared Initial Transport Revenue Recovery for

generation

ALF = Annual Load Factor appropriate to that generator.

1. Similar to the Peak Security background, the initial revenue recovery for gross GSP group demand for the Year Round background is calculated by multiplying the initial tariff by the total forecast metered triad gross GSP group demand:



Where:

ITRRDYR = Year Round Initial Transport Revenue Recovery for gross GSP

group demand

1. The initial revenue recovery for Embedded Exports is the Embedded Export Tariff multiplied by the total forecast volume of Embedded Export at triad:

Where

ITRREE = Initial Revenue impact for Embedded Exports

EEVDi = Forecast Embedded Export metered volume at Triad (MW)

For the avoidance of doubt, the initial revenue recovery for embedded exports

can be positive or negative.

## Deriving the Final Local Tariff (£/kW)

## *Local Circuit Tariff*

1. Generation with a local circuit tariff is calculated by multiplying the Year Round nodal marginal km along the local circuit by the expansion constant and the relevant local security factor (whether onshore or offshore) and summing across local circuits to give the local circuit tariff:



Where

*k* = Local circuit *k* for generator

NLMkmGjL = Year Round Nodal marginal km along local circuit *k* using local circuit expansion constant.

EC = Expansion Constant

LocalSF*k* = Local Security Factor for circuit *k*

CLTGi  = Circuit Local Tariff (£/kW)

### 

### **Onshore Local Substation Tariff**

1. All chargeable generation is subject to the local substation tariff component which is determined by assessing the generation substation type which is the substation at the connection charging boundary, against three cost determining factors:

(a) HV connection voltage – the voltage at the boundary between the User’s connection assets and the transmission system;

(b) Sum of TEC at the generation substation – the combined TEC of all generation at the connecting substation; and

(c) The level of redundancy at the generation substation – single busbar / single switch mesh connections are examples of no redundancy connections, whereas examples of connections with redundancy include double busbar and mesh sub station designs.

1. Using the above factors, the corresponding £/kW tariffs that are currently applicable, are detailed in The Company's **Statement of Use of System Charges** which is available from the **Charging website**.
2. The process for calculating Local Substation Tariffs will be carried out for the first year of the price control and will subsequently be indexed by TOPI for each subsequent year of the price control period.
3. The effective **Local Tariff** (£/kW) is calculated as the sum of the circuit and substation onshore and/or offshore components:



Where

ELTGi  = Effective Local Tariff (£/kW)

SLTGi  = Substation Local Tariff (£/kW)

1. Where tariffs do not change mid way through a **Financial Year**, final local tariffs will be the same as the effective tariffs:

ELTGi  = LTGi

Where

LTGi  = Final Local Tariff (£/kW)

1. Where tariffs are changed part way through the year, the final tariffs will be calculated by scaling the effective tariffs to reflect that the tariffs are only applicable for part of the year and parties may have already incurred TNUoS liability.

 and 

Where:

b = number of months the revised tariff is applicable for

FLL = Forecast local liability incurred over the period that the original tariff is applicable for

1. For the purposes of charge setting, the total local charge revenue is calculated by:



Where

LCRRG  = Local Charge Revenue Recovery

Gj = Forecast chargeable Generation or Transmission Entry Capacity in kW (as applicable) for each generator (based on analysis of confidential information received from Users)

### **Offshore substation local tariff**

1. All offshore chargeable generation is subject to an offshore substation tariff. The offshore substation tariff shall be the sum of transformer, switchgear and platform components.
2. Each tariff component, expressed in £/kW, shall be the ratio of the Offshore Transmission Owner revenue (£) and rating associated with the transformers, switchgear or platform (kW) at each offshore substation. The Offshore Transmission Owner revenue of each tariff component shall include that associated with asset spares. In the case of the platform component, the relevant rating shall be the lower of the transformer or switchgear ratings. As with the offshore circuit expansion constants, the Offshore Transmission Owner revenue associated with each tariff component shall be averaged over the remaining years of the NETSO price control.
3. Offshore Transmission Owner revenue associated with interest during construction and project development overheads will be attributed to the relevant asset category with which it is associated. If these or any other costs included in the Offshore Transmission Owner revenue are not readily attributable to a given asset category, they will be pro-rated across the various asset categories based on their relative cost.
4. A discount shall be provided to the offshore substation tariff to reflect the average cost of civil engineering for onshore substations. The currently applicable discount is detailed in The Company's **Statement of Use of System Charges** which is available from the **Charging website**. This will be inflated by TOPI each year and reviewed every price control period.
5. Offshore substation tariffs shall be reviewed at the start of every onshore price control period. For each subsequent year within the price control period, these shall be inflated in the same manner as the associated Offshore Transmission Owner Revenue.
6. The revenue from the offshore substation local tariff is calculated by:



Where:

SLTk = the offshore substation tariff for substation k

Genk = the generation connected to offshore substation k

1. [↑](#footnote-ref-2)